# bouvet/macropad/v1

![bouvet/macropad/v1](https://www.kefo.no/assets/macropad/macropad_v1.png)
Small macropad, with two rotary encoder buttons and 14 keys.
Optional OLED 128x16 screen, small learning and sharing project.

* Keyboard Maintainer: [Kenneth Fossen](https://github.com/spydx)
* Hardware Supported: Bouvet Macropad
* Hardware Availability: [Shop](https://www.kefo.no/macropad)

Make example for this keyboard (after setting up your build environment):

    make handwired/bouvet/macropad/v1:default

Flashing example for this keyboard:

    make handwired/bouvet/macropad/v1:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

## Bootloader

Enter the bootloader in 3 ways:

* **Bootmagic reset**: Hold down the key at (0,0) in the matrix (usually the top left key or Escape) and plug in the keyboard
* **Physical reset button**: Briefly press the button on the back of the PCB - some may have pads you must short instead
* **Keycode in layout**: Press the key mapped to `QK_BOOT` if it is available
